



|  |
| --- |
|  |

|  |
| --- |
| Guide for Upgrading NIC Card Firmware Using ISO Image Files |
| R1.0 |


1、Query the initial firmware version of the NIC card, which can be found out of band or in BIOS or Linux systems, for example:




2、Log in to the BMC for settings. Select service management - virtual media,Save the following configuration changes




3、Mount ISO image file. Select Virtual console -> Operate ->Start Java Virtual Console




Select Media - Virtual Media Wizard...




Select the firmware to be upgraded and click on connect




4、Perform ISO image upgrade. Select system management - system settings. Set up according to the following image, select CD/DVD drive, click save.



Reboot. If the upgrade is successful, you should see the following process. No operation is required.





5、Query the firmware version of the NIC card after rebooting, which can be found out of band or in BIOS or Linux systems, for example:

